
                              SILKSCREEN GENERATOR
                              --------------------

                          04:14 PM Monday, May 17, 2021
Job Name: Z:\project_non_backup\UT_Scintilla\LayoutWorkshop\Board_Design_VX2.7.2\Tx_Rx_433MHz_V2.0_start_training\PCB\Board1.pcb


    Silkscreen Side To Process           : TOP

    Process All Cell Types               : YES

    Top Silkscreen For Selected Cells    : Silkscreen Reference Designator Top
                                         : Silkscreen Outline Top
                                         : Sintecs_Logo_new
                                         : ESD_Symbol

    Break Silkscreen Using               : Soldermask Pads

    Break Graphics Pad Clearance         : 0.15mm

    Break Graphics Via Clearance         : 0.15mm

    Break Text Pad Clearance             : 0.15mm

    Break Text Via Clearance             : 0.15mm

    Broken Graphics Line Width           : 0.025mm

    Broken Text Line Width               : 0.15mm
    


    TOP Silkscreen Data Created Successfully (135 Geometries).