

|  |  |
| --- | --- |
| Terminal | Function |
| 1 | Positive end speaker (Red) |
| 2 | Negative end speaker (Black) |
| 3 | Negative voltage supply |
| 4 | Positive voltage supply |