
                            METAL BALANCING PROCESSOR
                            -------------------------

                         09:05 AM Friday, April 30, 2021
Job Name: C:\projects\UT_Scintilla\LayoutWorkshop\Design\VX2.7\Tx_Rx_433MHz_V1.1\PCB\Board1.pcb



    COMMON PARAMETERS
        Discard Areas By Dimension          : YES (10mm X 10mm)



        POSITIVE PLANE LAYER : 1

            Total Metal Balancing Shapes   : 1
            Metal Balancing Methodology    : Interactive

                Clearance                   : 0.75mm
                Offset X                    : 1.7mm
                Offset Y                    : 0mm
                Shape Width                 : 1.5mm
                Shape Distance              : 2mm
                Shape Pattern               : Diamond
                Metal Percentage            : 28.00



                        09:05 AM Friday, April 30, 2021